#include <WiFi.h>

const int ledPin = 2; // Set the LED pin

void setup() {

pinMode(ledPin, OUTPUT); // Initialize the LED pin as an output

}

void loop() {

digitalWrite(ledPin, HIGH); // Turn the LED on (HIGH is the voltage level)

delay(1000); // Wait for a second

digitalWrite(ledPin, LOW); // Turn the LED off by making the voltage LOW

delay(1000); // Wait for a second

}